Instruction for ADT686/673 U-Disk upgrade

1. Copy the update package to the root directory of the USB disk.
2. If it is a TYPE-C USB disk, insert the USB disk directly into the USB Type-C port on the back of the ADT686/673, as shown in Figure 1. If it is a TYPE-A USB disk, use the TYPE-C adapter in the accessories to insert the USB disk into the device, as shown in Figure 2.

****

**Figure 1 Insert a TYPE-C USB disk directly**

****


**Figure 2 Insert the TYPE-A USB disk by a TYPE-C adaptor**

1. Click the icon  at the bottom of the main page, as shown in Figure 3.



**Figure 3 Enter the function menu**

1. Select “Set up”, as shown in Figure 4.




**Figure 4 Set up**

1. Select “Service”, as shown in Figure 5.



**Figure 5 System service**

1. Select “System update” in the service page, then click “U-Disk upgrade” to update the firmware, as shown in the Figure 6.



**Figure 6 U-Disk upgrade**

1. After entering the upgrade, if there are several update packages in the USB disk, the system will prompt the user to select the package to be updated. After that, the system will start to reading the package, and then show the firmware information in the update package. Users need to confirm to start the firmware update. After the update is completed, the result of each component will be shown, and the device will automatically restart after a confirmation.